**Enduromax DCC2003SM/36/SV Overhead Door Closer**



**Product Details**

Suitable for Industrial, Domestic or Commercial Use

Dimensions: 236mm x 59mm

Available Finishes:

     - Silver Standard (Without Cover Plate)
     - Electro Brass (Door closer and Plated arm, Fixings and Cover pack)
     - Polished Nickel Plated (Door closer and Plated arm, Fixings and Cover pack)
     - Satin Nickel Plated (Door closer and Plated arm, Fixings and Cover pack)
     - Silver (Door closer and Plated arm, Fixings and Cover pack)

Closing Force EN Size 3

Efficiency 77%

Max Door Width: 950mm

Max Weight: 60Kg

Angle Of Opening Max 120 Degrees

Suitable For Left Hand Or Right Hand Use

Adjustable Closing Speed

Adjustable Latching Speed

10 year Mechanical Guarantee

Slide Channel

Slimline Body

Suitable for Fire Doors Rated to FD30/60/120/240

Meets Recommendations Of BS 8300 (DDA Compliant)