**ASTRA DOOR CONTROLS**

AST3003 Door Control – Technical Data

Product:

* Integrated door control
* Jamb mounted frame plate hinge side
* Suitable for use on right and left swing doors
* Completely concealed when door is closed

Performance

* Fixed power EN3
* Closing force 4° from latch 19Nm
* Opening force 4° from latch 22Nm
* Continuous valve control from 90°
* Maximum opening angle 105°

Functions

* Adjustable closing speed whilst installed
* Adjustable latching action
* Maintenance free

Test Evidence

* Continuous testing 500,000 cycles
* Included in Enhanced Security Door-set to PAS24 Sound Secure Range Halspan and Strebord 44mm and 54mm fire doors
* Fire test conducted in accordance with BS EN1634-1:2000 Test report CHILT/RF06118
* Tested to European Harmonised Standard BS EN1154

Accreditations

* CE marked in accordance with the Construction Products Regulation (CPR)
* CERTIFIRE approved Supplement to Certificate numbers CF195, CF198, CF240, CF240A, CF241, CF302, CF380 and CF625 Supplement number 357429
* PAS24 (Secured By Design) Certificate 050/002